FieldTalk Modbus Master Library for .NET
FieldTalk Modbus Master Library for .NET
Namespaces
FieldTalk.Modbus.Master
MbusMasterFunctions Class
MbusMasterFunctions Methods
configureStandard32BitMode Method
configureStandard32BitMode Method
configureStandard32BitMode Method (Int32)

# MbusMasterFunctions configureStandard32BitMode Method (Int32)

Configures a slave for Standard 32-bit Mode.

Namespace: FieldTalk.Modbus.Master
Assembly: FieldTalk.Modbus.Master (in FieldTalk.Modbus.Master.dll) Version: 2.15.2-eval+3d8362b4bb861c05760d48b11d303e954bb8597c
Syntax
C#
VB
C++
Copy

    public int configureStandard32BitMode(
    	int slaveAddr
    )

    Public Function configureStandard32BitMode (
    	slaveAddr As Integer
    ) As Integer

    public:
    int configureStandard32BitMode(
    	int slaveAddr
    )

#### Parameters

slaveAddr
  Type: System
  Int32
  Modbus address of slave device or unit identifier (Range: 1 - 255) A value of zero configures the behaviour for broadcasting.

#### Return Value

Type: Int32
BusProtocolErrors.FTALK_SUCCESS on success or BusProtocolErrors.FTALK_ILLEGAL_ARGUMENT_ERROR if argument out of range
Remarks
In Standard 32-bit Register Mode a 32-bit value is transmitted as two consecutive 16-bit Modbus registers.

Note
This function call also re-configures the endianess to default little-endian for 32-bit values!

Note
This is the default mode.

See Also

#### Reference

MbusMasterFunctions Class
configureStandard32BitMode Overload
FieldTalk.Modbus.Master Namespace
FieldTalk Modbus Master Library for .NET
Library version 2.15.2