FieldTalk Modbus Master Library for .NET
FieldTalk Modbus Master Library for .NET
Namespaces
FieldTalk.Modbus.Master
MbusMasterFunctions Class
MbusMasterFunctions Properties
pollDelay Property
retryCnt Property
timeout Property

# MbusMasterFunctions pollDelay Property

Poll delay property

Namespace: FieldTalk.Modbus.Master
Assembly: FieldTalk.Modbus.Master (in FieldTalk.Modbus.Master.dll) Version: 2.15.2-eval+3d8362b4bb861c05760d48b11d303e954bb8597c
Syntax
C#
VB
C++
Copy

    public int pollDelay { get; set; }

    Public Property pollDelay As Integer
    	Get
    	Set

    public:
    property int pollDelay {
    	int get ();
    	void set (int value);
    }

#### Property Value

Type: Int32
Delay value in ms (Range: 0 - 100000), 0 disables poll delay
Remarks
This property sets the delay time which applies between two consecutive Modbus read/write. A value of 0 disables the poll delay.

The delay value is indicative only and not guaranteed to be maintained. How precise it is followed depends on the operating system used, it's scheduling priority and it's system timer resolution.

Note
A protocol must be closed in order to configure it.

See Also

#### Reference

MbusMasterFunctions Class
FieldTalk.Modbus.Master Namespace
FieldTalk Modbus Master Library for .NET
Library version 2.15.2