FieldTalk Modbus Master Library for .NET
FieldTalk Modbus Master Library for .NET
Namespaces
FieldTalk.Modbus.Master
MbusMasterFunctions.FileSubRequest Structure
FileSubRequest Fields
fileNo Field
recordArr Field
recordNo Field
refType Field

# FileSubRequest Fields

The MbusMasterFunctions
FileSubRequest type exposes the following members.

Fields

| Name | Description
--- | --- | ---
| fileNo | File number (Range 1-65535). 3 is the input registers file, 4 is the holding registers file.
| recordArr | Pointer to a buffer which will be filled with the data read or contains the data to be sent.
| recordNo | Record Number (Range: 0 - 65535). The first record (aka register) to read from, 0-based numbering.
| refType | Reference type (Must be specified as 6).

Top
See Also

#### Reference

MbusMasterFunctions
FileSubRequest Structure
FieldTalk.Modbus.Master Namespace
FieldTalk Modbus Master Library for .NET
Library version 2.15.2